**What is the pipe strap ?**

**Introduction：**

One hole or two hole Rigid Conduit Strap is used for securing EMT (Electrical Metallic Tube) , IMC or galvanized rigid conduit (GRC),SS201& SS304 to wood or masonry. The zinc-plated steel is corrosion resistant. Used for interior and exterior use.The straps have a high load-bearing capacity and snap onto the conduit to hold it securely in place.

**Pipe Strap Sizes:**

* Available Material: Galvanized ,SS201 ,SS304
* Usual size :5/8” , 3/4”,1”, 1-1/4”,1-1/2”,2” etc.for one hole and 1/2”,5/8”,3/4”，
* 1”,1-1/4”,1-1/2”,2” ect. for two hole .

**Features and advantages :**

* Secures rigid or IMC conduit to wood, masonry and other surfaces
* For Greater load
* Good performance for anti corrosion .
* Packing will be box + carton+pallet .

**Installation：**

**Attach fittings to the wall:**  using screws and straps with either single hole or double holes to attach electrical conduit fittings to the wall ,masonry or the other surface .

****